Put a breakpoint at \_\_\_\_\_\_\_\_\_\_\_\_\_

Set up so PORT B, pin 3 can go fired to low, but don’t fire it

Run to line \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Fire (Trigger) PORT B, pin 3

Step Once

Show me the value of \_\_\_\_\_\_

Show it to me another way

Show me the value of w

Show me the value of the Carry flag

Show me the value of the Zero flag

Show me the value of **program memory** location 32

Show me the value of file register at 31Hex

If the Dip Switch is Up, is the input LOW or HIGH?